SIA “Rīgas Austrumu klīniskā universitātes slimnīca”

Tehniskā specifikācija – finanšu piedāvājums
Cenu aptaujai
Video tehnikas iegāde

	Npk.
	Pozīcija
	Tehniskie parametri
	Pretendenta piedāvātā cena

	1.
	Videokamera
	
	

	
	LENS SECTION
	F Value
	F1.8 ― 4.0
	

	
	
	Optical Zoom
	24x
	

	
	
	Focal Length
	4.12 ― 98.9mm
	

	
	
	35 mm Film Camera Equivalent
	25.0 ― 600.0 mm
	

	
	
	Filter Diameter
	62 mm
	

	
	CAMERA SECTION
	Minimum Illumination
	1.5 lx (F1.8, Super Gain +, 1/30)
	

	
	
	Focus
	Auto / Manual
	

	
	
	Intelligent Zoom OFF
	24x
	

	
	
	Intelligent Zoom ON
	Max. 48x (UHD 32x)
	

	
	
	Digital Zoom
	2x / 5x / 10x
	

	
	
	ND Filter
	1/4, 1/16, 1/64, OFF
	

	
	
	IR Filter
	Incorporates the ON/OFF control function
	

	
	
	White Balance
	Auto / ATW LOCK / 3200K / 5600K / VAR (2000K—15000K) / Ach Fixed / Bch Fixed
	

	
	
	Shutter Speed - 59.94 Hz mode
	59.94i/59.94p: 1/60, 1/100, 1/120, 1/180, 1/250, 1/350, 1/500, 1/750, 1/1000,
1/1500,1/2000, 1/3000, 1/4000, 1/8000 sec
29.97p: 1/30, 1/50, 1/60, 1/100, 1/120, 1/180, 1/250, 1/350, 1/500, 1/750, 1/1000,
1/1500,1/2000, 1/3000, 1/4000, 1/8000 sec
23.98p: 1/24, 1/48, 1/50, 1/60, 1/100, 1/120, 1/180, 1/250, 1/350, 1/500, 1/750,
1/1000, 1/1500, 1/2000, 1/3000, 1/4000, 1/8000 sec
	

	
	
	Shutter Speed - 50.00 Hz mode
	50i/50p: 1/50, 1/60, 1/100, 1/125, 1/180, 1/250, 1/350, 1/500, 1/750, 1/1000, 1/1500, 1/2000,
1/3000, 1/4000, 1/8000 sec
25p: 1/25, 1/50, 1/60, 1/100, 1/125, 1/180, 1/250, 1/350, 1/500, 1/750, 1/1000, 1/1500, 1/2000,
1/3000, 1/4000, 1/8000 sec
	

	
	
	Slow Shutter Speed - 59.94 Hz mode
	59.94i/59.94p: 1/8, 1/15, 1/30 sec
29.97p: 1/8, 1/15 sec
23.98p: 1/6, 1/12 sec
	

	
	
	Slow Shutter Speed - 50.00 Hz mode
	50i/50p: 1/6, 1/12, 1/25 sec
25p: 1/6, 1/12 sec
	

	
	
	Super Slow Recording Frame Rate - 59.94 Hz mode
	FHD 120 fps (1/2 speed at 60p, 1/4 speed at 30p, 1/5 speed at 24p)
	

	
	
	Super Slow Recording Frame Rate - 50.00 Hz mode
	FHD 100 fps (1/2 speed at 50p, 1/4 speed at 25p)
	

	
	
	Iris
	Auto / Manual
	

	
	
	Image Stabilizer
	Ball O.I.S., 5-Axis HYBRID O.I.S. (UHD/FHD)
	

	
	RECORDING SECTION
	Recording Media
	SDHC/SDXC Memory Card
	

	
	
	Recording Format
	MOV, MP4, AVCHD
	

	
	
	Video Compression Method
	MOV/MP4: H.264/MPEG-4 AVC High Profile, H.265/MPEG-H HEVC Main10 Profile
AVCHD: H.264/MPEG-4 AVC High Profile
	

	
	
	Audio Compression Method
	MOV: LPCM (24bit 2ch)
MP4: AAC (16bit 2ch)
AVCHD: Dolby Audio (16bit 2ch)
	

	
	
	System Frequency
	59.94Hz / 50.00Hz
	

	
	
	Recording / Playback Mode
	MOV (HEVC), MOV, MP4 (HEVC), MP4, AVCHD
	

	
	LIVE STREAMING
	Video Compression Format
	
H.264/MPEG-4 AVC Main Profile, High Profile

	

	
	
	Video Resolution
	1920 x 1080 (FHD), 1280 x 720 (HD), 640 x 360, 320 x 180
	

	
	
	Streaming Method
	Unicast, Multicast
	

	
	
	Frame Rate
	System frequency = 59.94 Hz: 30 fps, 60 fps
System frequency = 50.00 Hz: 25 fps, 50 fps
	

	
	
	Bit Rate
	4 Mbps, 20 Mbps, 16 Mbps, 14 Mbps, 8 Mbps, 6 Mbps, 4 Mbps, 3 Mbps, 2 Mbps, 1.5 Mbps, 1 Mbps, 0.7 Mbps, 0.5 Mbps
	

	
	
	Audio Compression Format
	AAC-LC, 48 kHz/16 bit, 2ch
	

	
	
	Network Protocol
	RTSP/RTP/RTMP/RTMPS
	

	
	STILL IMAGE SECTION
	Recording Format
	JPEG (DCF/Exif2.2)
	

	
	
	Recording Image Size
	Video Playback Mode: 3840 x 2160 (16:9), 1920 x 1080 (16:9), 1280 x 720 (16:9)
	

	
	GENERAL SECTION
	Power Supply
	7.28V (Battery) / 12V (AC Adaptor)
	

	
	
	Power Consumption
	15.5W (LCD Monitor)
	

	
	
	Weight
	Up to 2 kg
	

	
	
	LCD Monitor
	3.5-inch Wide LCD monitor (About 2,760,000 dots)
	

	
	
	Viewfinder
	0.24-inch Wide EVF (About 1,560,000 dots)
	

	
	
	Manual Ring
	Focus / Zoom or Iris
	

	
	
	Accessory Shoe
	Yes
	

	
	
	LED Video Light Average Illumination
	Approx. 70 lx (1.0m)
	

	
	
	LED Video Light Irradiation Angle
	Approx. 30°
	

	
	
	LED Video Light
	Approx. 4600K
	

	
	INTERFACE SECTION
	Video SDI OUT
	BNC x 1, 0.8V[p-p], 75Ω, 3G/1.5G HD-SDI supported
Output format:
1080/59.94p LEVEL-A/50.00p LEVEL-A, 1080/29.97PsF/25.00PsF/23.98PsF, 1080/59.94i/50.00i, 720/59.94p/50.00p
	

	
	
	Video HDMI
	Type A x 1 (VIERA Link not supported)
Output format:
2160/59.94p/50.00p/29.97p/25.00p/23.98p,
1080/59.94p/50.00p/29.97p/25.00p/23.98p/59.94i/50.00i,
720/59.94p/50.00p, 480/59.94p, 576/50.00p
	

	
	
	Audio Input
	Built-in Microphone - Stereo microphone
	

	
	
	
	Microphone Input - 3.5mm stereo mini jack x 1
	

	
	
	
	XLR Input - XLR (3 pins) x 2
Input high impedance, LINE/MIC/MIC+48 V (switchable SW)
LINE：+4dBu/0dBu (switchable menu)
MIC: –40dBu/–50dBu/–60dBu (switchable menu)
	

	
	
	Audio Output
	SDI - 2 ch (LPCM) Gain: 0dB/-6dB/-8dB
	

	
	
	
	HDMI - 2 ch (LPCM 24bit)
	

	
	
	
	Headphone - 3.5 mm diameter stereo mini jack x 1
	

	
	
	
	Speaker - 15 mm diameter, round x 1
	

	
	
	Other Input/Output
	Camera Remote - 2.5mm super mini jack x 1
	

	
	
	
	USB 2.0 DEVICE - Micro-AB connector, 5-pin, mass storage function
	

	
	
	
	DC IN - DC 12V (11.4V ― 12.6V) EIAJ Type4
	

	
	
	Wi-Fi
	Standard - IEEE 802.11b/g/n
	

	
	
	
	Frequency - 2.4GHz band
	

	
	STANDARD ACCESSORY
	AC Adaptor
	Yes
	

	
	
	AC Cable
	Yes
	

	
	
	Rechargeable Battery Pack
	Yes (5,900mAh)
	

	
	
	Handle Unit
	Yes (detachable)
	

	
	
	Microphone Holder
	Yes
	

	
	
	Microphone Holder Screws
	Yes
	

	
	
	Eye Cup
	Yes
	

	
	
	Lens Hood
	Yes
	

	
	
	
	

	2.
	Statīvs 
	Payload
	4 kg
	

	
	
	Counterbalance
	FIX
	

	
	
	Drag mode
	FIX
	

	
	
	Tilt angle
	+90° / -80°
	

	
	
	Temperature range
	-20°C to +60°C
	

	
	
	Bubble level
	Non illuminated
	

	
	
	Camera plate
	Sliding plate
Compatible with Manfrotto and Sachtler heads
	

	
	
	Sliding range
	+/-30mm / 1.2"
	

	
	
	Plate attachment
	1/4" screw with video pin
	

	
	
	Weight
	3.1 kg
	

	
	
	Height
	75.5cm to 159cm 
	

	
	
	Ball diameter
	65mm
	

	
	
	Section
	2STAGE
	

	
	
	
	

	3.
	Bezvadu mikrofons
	Color
	Black 
	

	
	
	Frequency response
	20 Hz - 20000 Hz
	

	
	
	THD, total harmonic distortion
	typ. 0.1 %
	

	
	
	Weight
	Receiver: 87 g (incl energy pack)
	

	
	
	Audio input
	3,5 mm mini jack
	

	
	
	Audio output
	XLR
	

	
	
	Operating temperature
	-10 °C - + 55°C
	

	
	
	Signal-to-noise ratio
	> 90 dB(A)
	

	
	
	RF output power
	adaptive up to 250mW (peak) country specific
	

	
	
	Operating time
	> 4h (Receiver), typ 15 h (Transmitter with LiIon energy pack)
	

	
	
	Modulation
	GFSK (DECT)
	

	
	
	Audio output level
	-30 dBu - 0 dBu in 4 Steps
	

	
	
	Battery Specification
	Li-Ion 3,7 V DC
	

	
	
	Dynamic range
	> 120 dB(A)
	

	
	
	Frequency band
	1880 - 1930 MHz (Country specific)
	

	
	
	Sampling rates
	24 bit / 48 kHz
	

	
	
	Latency
	19 ms
	

	
	
	Atbilstība radio frekvenču ES standartiem
	Jā
	

	
	
	
	

	4.
	Atmiņas kartes
	Skaits
	2 gab.
	

	
	
	Capacity
	128 GB
	

	
	
	Compatibility
	Compatible with SDXC and SDXC UHS-I enabled host devices
	

	
	
	Dimensions (L x W x H)
	31.92mm x 23.91mm x 2.17mm
	

	
	
	
	

	5.
	Kameras Mikrofons 
	Dimensions
	Diameter 20 mm, length 256 mm
	

	
	
	Microphone
	Super-cardioid/lobar 
	

	
	
	Frequency response
	40 Hz to 20 kHz
	

	
	
	Max. sound pressure level
	132 dB SPL at P48; 126 dB SPL with battery powering
	

	
	
	Weight
	128 g (without battery)
	

	
	
	Sensitivity in free field, no load (1kHz)
	21 mV/Pa at P48; 19mV/Pa with battery powering
	

	
	
	Equivalent noise level
	15 dB (A) at P48; 16 dB (A) with battery powering
	

	
	
	Operating time
	approx. 150 hrs
	

	
	
	Power supply
	48 V +/- 4V (P48, IEC 61938) or battery/rechargeable batt. 1,5V/1,2V AA size
	

	
	
	Current consumption
	4,4 mA at P48
	

	
	
	
	



Piegādes termiņš – 10 darba dienas.
Piedāvājumā jāiekļauj arī visas ar piegādi saistītās izmaksas. Apmaksa ar pēcapmaksu.
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