Cenu aptauja
“Kabeļu un materiālu iegāde”
Tehniskā specifikācija
	Npk.
	Pozīcija
	Tehniskie parametri
	Pretendenta piedāvājums

	1.
	Sadales kārba priekš vītā pāra kabeļa
	· CAT 5e and CAT 6;
· Connection over LSA strips;
· Integrated strain relief;
· Shielded.
	

	
	
	Material enclosure
	ABS non halogen
	

	
	
	Cable entry
	Up to 6.8 mm
	

	
	
	[bookmark: _GoBack]Temperature range
	-40°C up to +80 °C
	

	

	2.
	CAT 5e Patch panelis
	· Unshielded, rack mount, color black (RAL 9005), 24-port;
· ISO/IEC 11801 and EN 50173;
· RJ45 jacks, 8P8C;
· Material housing: SECC, 1.5 mm galvanized;
· Cable installation via LSA strips;
· Fixing option for cable ties, central ground connection;
· Suitable for 483 mm (19") rack mount.
	

	

	3.
	Vītā pāra datu kabelis
	CAT 5e Class D, U/UTP, Twisted Pair Installation Cable, 100 MHz
	

	
	
	Application areas: Primary (Campus), Secondary (Riser), Tertiary (Horizontally) IEEE 802.3: 10Base-T; 100Base-T; 1000Base-T IEEE 802.5: 16 MB; ISDN; FDDI; ATM; PoE
	

	
	
	Standards: ISO/IEC 11801 3rd Ed.; EN 50173-1/4; EN 50288-3-1; IEC 61156-5
	

	
	
	Length/Packaging - 305 m box, simplex
	

	
	
	Physical Properties
	

	
	
	Total number of insulated conductors
	8, twisted in 4 pairs
	

	
	
	Color code
	Blue-white, orange-white, green-white, brown-white
	

	
	
	Individual pair shielding
	None
	

	
	
	Overall shielding
	None
	

	
	
	Outer sheath
	ECA acc. to EN 50575; PVC
	

	
	
	Outer sheath diameter (nominal)
	0.50 mm nominal
	

	
	
	Outer sheath color
	Grey
	

	
	
	Mechanical Properties
	

	
	
	Tensile loading
	150 N max.
	

	
	
	Dynamic bending radius
	8x AD mm min.
	

	
	
	Static bending radius
	4x AD mm min.
	

	
	
	Operating temperature range
	-20 °C up to +60 °C
	

	
	
	Installations temperature range
	0 °C up to +50 °C
	

	
	
	Overall diameter Simplex (nominal)
	4.7 mm nominal
	

	
	
	Electrical Properties
	

	
	
	Impedance
	100 ± 5 Ohm @ 1-600 MHz
	

	
	
	Capacitance
	40 pF/m nominal @ 800 KHz
	

	
	
	Capacitance unbalance (pair-ground)
	1.5 pF/m max. @ 1 KHz
	

	
	
	DC resistance
	72 Ohm/km max. (2% max. resistance unbalance)
	

	
	
	DC loop resistance
	147 Ohm/km max. (2% max. resistance unbalance)
	

	
	
	Voltage resistance
	72 Vdc max.
	

	
	
	Signal propagation delay
	535 nS/100 m max.
	



Finanšu piedāvājums
	
	Cena par gab. bez PVN
	Skaits
	Summa bez PVN
	Summa ar PVN

	Sadales kārba priekš vītā pāra kabeļa
	
	300
	
	

	CAT 5e Patch panelis
	
	20
	
	

	Vītā pāra datu kabelis
	
	30 kastes (9150m)
	
	

	
	
	Kopā:
	



Piedāvājumā jāiekļauj visas izmaksas, kas saistītas ar piegādes un transporta izmaksām.
Piegādes termiņš – 15 darba dienas.
