Tehniskā specifikācija
[bookmark: _GoBack]Audio aprīkojuma iegāde
	N.p.k.
	Pozīcija
	Tehniskie parametri
	Pretendenta piedāvājums

	1.
	Datora ārējā audio iekārta
	FOCUSRITE Scarlett 2i2 3rd Gen vai līdzvērtīgs
	

	
	
	SUPPORTED SAMPLE RATES
	44.1kHz, 48kHz, 88.2kHz, 96kHz, 176.4kHz, 192kHz
	

	
	
	MICROPHONE INPUTS
	

	
	
	Frequency Response
	20Hz - 20kHz ± 0.1dB
	

	
	
	Dynamic Range
	111dB (A-weighted)
	

	
	
	THD+N
	<0.0012% 
	

	
	
	Noise EIN
	-128dBu (A-weighted)
	

	
	
	Maximum Input Level
	9dBu (at minimum gain)
	

	
	
	Gain Range
	56dB
	

	
	
	Impedance
	3kΩ
	

	
	
	LINE INPUTS
	

	
	
	Frequency Response
	20Hz - 20kHz ± 0.1dB
	

	
	
	Dynamic Range
	110.5dB (A-weighted)
	

	
	
	THD+N
	<0.002%
	

	
	
	Maximum Input Level
	22dBu (at minimum gain)
	

	
	
	Gain Range
	56dB
	

	
	
	Impedance
	60kΩ
	

	
	
	INSTRUMENT INPUTS
	

	
	
	Frequency Response
	20Hz - 20kHz ± 0.1dB
	

	
	
	Dynamic Range
	110dB (A-weighted)
	

	
	
	THD+N
	<0.03%
	

	
	
	Maximum Input Level
	12.5dBu (at minimum gain)
	

	
	
	Gain Range
	56dB
	

	
	
	Impedance
	1.5MΩ
	

	
	
	LINE/MONITOR OUTPUTS
	

	
	
	Dynamic Range (Line Outputs)
	108dB
	

	
	
	THD+N
	<0.002%
	

	
	
	Maximum Output Level (0 dBFS)
	15.5dBu
	

	
	
	Impedance
	430Ω
	

	
	
	HEADPHONE OUTPUTS
	

	
	
	Dynamic Range
	104dB (A-weighted)
	

	
	
	THD+N
	<0.002%
	

	
	
	Maximum Output Level
	7dBu
	

	
	
	Impedance
	<1Ω
	

	
	
	Warranty
	2 years
	

	2.
	Mikrofons
	IMG STAGE LINE HSE-152/SK vai līdzvērtīgs
	

	
	
	Description
	headband microphone
	

	
	
	Transmission method
	cable
	

	
	
	Polar pattern
	cardioid
	

	
	
	System
	back electret
	

	
	
	Audio frequency range
	20-20,000 Hz
	

	
	
	Nominal impedance
	1 kΩ
	

	
	
	Sensitivity
	8 mV/Pa
	

	
	
	Max. sound pressure
	130 dB
	

	
	
	Power supply
	DC 1.5-9 V
	

	
	
	Connection
	3-pole mini XLR
	

	
	
	Admiss. ambient temp.
	0-40 °C
	

	
	
	Warranty
	2 years
	

	3.
	Radio mikrofona komplekts
	DB TECHNOLOGIES RW16 BS vai līdzvērtīgs
	

	
	
	Battery type
	AA
	

	
	
	Frequency suitable for EU
	Yes, no licence required
	

	
	
	Frequency band
	dB technologies Band 6 (823 - 832 MHz)
	

	
	
	Includes headset
	yes
	

	
	
	Channel
	65 (822 - 830 MHz), 66 (830 - 838 MHz)
	

	
	
	Maximum frequency
	15 - 15.9 kHz
	

	
	
	Minimum frequency
	60 - 79 Hz
	

	
	
	Polar pattern
	cardioid
	

	
	
	Type of frequency band
	VHF (30 - 470 MHz)
	

	
	
	Power adapter
	ungrounded flat Europlug
	

	
	
	Warranty
	2 years
	



Finanšu piedāvājums
	N.p.k.
	Pozīcija
	Skaits
	Cena gab. bez PVN
	Cena gab. ar PVN

	1.
	Datora ārējā audio iekārta
	2 gab.
	
	

	2.
	Mikrofons
	2 gab.
	
	

	3.
	Radio mikrofona komplekts
	2 gab.
	
	

	
	
	Kopā:
	
	



Piedāvājumā jāiekļauj visas izmaksas, kas saistītas ar piegādes un transporta izmaksām.
Piegādes termiņš – viss apjoms 1 piegādē – 14 dienu laikā, no apstiprinājuma e-pasta saņemšanas par konkursa rezultātiem.

