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	Termodrukas aproču printeris
	Printer Specifications
	Resolution: 203 dpi/8 dots per mm
Optional 300 dpi/12 dots per mm
Memory;	512 MB Flash; 256 MB SDRAM
Maximum Print Width:	2.2 in./56 mm for 203 dpi and 300 dpi
Maximum Print Speed;	6 in./152 mm per second (203 dpi) 4 in./102 mm per second (300 dpi)
Media Sensors:	Full width, moveable reflective/black mark sensor; multi-position transmissive/ gap sensor
Firmware: ZPL II; EPL 2; EPL Line Mode; XML; ZBI
	

	
	
	Media Specifications
	Maximum Label Length: 39.0 in./991 mm
Maximum Label and Media: Width2.36 in./60 mm
Media Roll Size:5.00 in./127 mm outer diameter
Core inner diameter: 0.5 in. (12.7mm) and 1.0 in. (25.4mm) standard, 1.5 in. (38.1mm), 2.0 in., (50.8mm) and 3.0 in. (76.2mm) using optional adapters
Thickness: 0.003 in. (0.08 mm) min. - 0.0075 (.1905 mm)
Media Types: Roll-fed or fan-fold, die cut or continuous direct thermal labels with or without black mark, tag stock, continuous receipt paper, and wristbands

	

	
	
	Label Roll Capacity
	165 mm (6.5“) OD
	

	
	
	Label Length
	10 ~ 2,286 mm (0.39“ ~ 90“)
	

	
	
	Internal Fonts
	16 resident expandable ZPL II bitmap fonts, two resident scalable ZPL fonts, five resident expandable EPL2 fonts, native open-type font support, Unicode compliant. China units include SimSun simplified Chinese font 64 MB user available non-volatile memory, 8 MB user available SDRAM
	

	
	
	Barcodes
	1D Barcodes: Code 11, Code 39, Code 93, Code 128, ISBT-128, UPC-A, UPC-E, EAN-8, EAN-13, UPC and EAN 2-or 5-digit extensions, Plessey, Postnet, Standard 2-of-5, Industrial 2-of-5, Interleaved 2-of-5, Logmars, MSI, Codabar and Planet Code
2D Barcodes: Codablock, PDF417, Code 49, DataMatrix, MaxiCode, QR Code, MicroPDF, Aztec
	

	
	
	Interface
	USB 2.0Internal Ethernet, 10/100 Mbps
USB host, for scanner or PC keyboard (factory option)
	

	
	
	Sensors
	Transmissive gap sensor Black mark reflective sensor (position adjustable)
Head open sensor
	

	
	
	Accessories
	USB cable, Power cord
External universal switching power supply
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	1.
	Termodrukas aproču printeris
	9 gab.
	
	
	
	



Piedāvājumā jāiekļauj visas izmaksas, kas saistītas ar piegādes un transporta izmaksām.
Piegādes termiņš – viss apjoms 1 piegādē – 14 dienu laikā, no apstiprinājuma e-pasta saņemšanas par konkursa rezultātiem.

