Tehniskā specifikācija
Termodrukas aproču printeru iegāde, TSC TDP-225W vai līdzvērtīgs
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	Termodrukas aproču printeris
	Printer Specifications
	Print Method: Direct Thermal
Resolution: 8 dots/mm (203 DPI)
Max. Print Speed: 127 mm (5”)/second
Max. Print Width: 52 mm (2.05“)
Max. Print Length: 2,286 mm (90“)
Processor: 32-bit RISC CPU
Memory: 4 MB Flash memory / 8 MB SDRAM / microSD card reader for Flash memory expansion, up to 4 GB
LCD: Graphic type, 128 x 64 pixels, with back light
	

	
	
	Media Specifications
	Media Type: Continuous, die-cut, black mark, fan-fold, notched, wristband (outside wound)
Media Width: 15 ~ 52 mm (0.59“ ~ 2.05“)
Media Thickness: 0.06 ~ 0.19 mm (2.36 ~ 7.48 mil)
Media Core Diameter: 25.4 mm (1”)
	

	
	
	Label Roll Capacity
	165 mm (6.5“) OD
	

	
	
	Label Length
	10 ~ 2,286 mm (0.39“ ~ 90“)
	

	
	
	Internal Fonts
	8 alpha-numeric bitmap fonts
Monotype Imaging® true type font engine with one CG Triumvirate Bold Condensed scalable font
	

	
	
	Barcodes
	1D bar code: Code 39, Code 93, Code 128UCC, Code 128 subsets A, B, C, Codabar, Interleave 2 of 5, EAN-8, EAN- 13, EAN-128, UPC-A, UPC-E, EAN and UPC 2 (5) digits add-on, MSI, PLESSEY, POSTNET, China POST, GS1 DataBar, Code 11
2D bar code: PDF-417, Maxicode, DataMatrix, QR code, Aztec
	

	
	
	Interface
	USB 2.0
Internal Ethernet, 10/100 Mbps
USB host, for scanner or PC keyboard (factory option)
	

	
	
	Sensors
	Transmissive gap sensor
Black mark reflective sensor (position adjustable)
Head open sensor
	

	
	
	Accessories
	USB cable, Power cord
External universal switching power supply
	



Finanšu piedāvājums
	N.p.k.
	Pozīcija
	Skaits
	Cena gab. bez PVN
	Cena gab. ar PVN
	Summa bez PVN
	Summa ar PVN

	1.
	Termodrukas aproču printeris
	20 gab.
	
	
	
	



Piedāvājumā jāiekļauj visas izmaksas, kas saistītas ar piegādes un transporta izmaksām.
Piegādes termiņš – viss apjoms 1 piegādē – 14 dienu laikā, no apstiprinājuma e-pasta saņemšanas par konkursa rezultātiem.
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